
***A horse trailer parked on a road

Description automatically generatedA white metal mesh on top of a vehicle

Description automatically generatedA trailer with open doors

Description automatically generated***

***2 HAL STANDARD – SQUARE - $22,995***

|  |  |
| --- | --- |
| **Specification** | * **2HAL – S SQUARE** |
| **Construction Materials** | * **Chassis: Double Hot Dip Galvanized RHS 3.5mm-4.0mm** * **Frame: Double Hot Dip Galvanized RHS (2.5mm)** * **Body Panels: Galvanized sheet (1.5mm)** * **Roof: Special Molded FRP Fiber-reinforced Polymer - Glassfibre (3mm)** |
| **BRAKES** | * **Double Axle Electric Brakes, with Security Brake Away System, rated to 1000kgs per Drum** |
| **DRAWBAR** | * **Drawbar Checker Plate 1.2mm High Strength Aluminum** * **Double Drawbar Safety Chains & One Bracing Wheel** |
| **Suspension** | * **7 Plate Roll Rocker Tandem Spring, With Grease Nipples** |
| **Axles** | * **Twin HD Trailer Axles 50\*50, rated to 2000kgs each.** |
| **Wheels & Tyres** | * **5 x 185 R14 tyres with 14' aluminum alloy rims including a lockable spare wheel** |
| **Flooring & Rubber Matting** | * **Re-enforced Aluminum Flooring, Covered with 18-20mm Anti Slip Rubber** * **Rubber Matting for Inner Side Panel, 6mm Rubber Matting** * **Rubber Matting for Floor & Ramp Door, 18-20mm Anti-Slip Rubber Matting** |
| **Windows & Doors** | * **Front Window 1220x610mm** * **4 Side Sash Windows 600mmx400mm, With Fly Screens** * **2 large Push-up Roof Vents** * **Rear Upper Door 1980x1065mm. 2 x High-strength anti-rust struts** * **Ramp Door 2030x1210mm, with anti-slip rubber matting** * **Side Door 1730x615mm** * **Hinges for Rear Upper Door - 6mm diameter Copper hinges** |
| **Supporting Wheel** | * **Swing-up HD Knight Dolly wheel** |
| **Lights& Retro Reflectors** | * **Trailer Plug - Seven prong.** * **Aluminum Rear Lights Brackets** * **2 x small LED sidelights, 2 x LED combination taillights** * **8 x Retro Reflectors** * **Fully adjustable bays 2,400mm long** |
| **Standard Auxiliary Fittings** | * **1 x large steel swing out tack box.** * **1 x rug racks over rear** * **Fully adjustable bays, 2400mm long** * **Removable stallion bars** |
| **Dimensions** | * **Body Dimension (L x W x Hmm) : 3260 x 1980 x 2230** * **Inner Dimension (L x W x Hmm) : 3290 x 1930 x 2155** * **Overall Dimension (L x W x Hmm): 4220 x 2490 x 2600** * **Length of Tow: 850mm** |
| **Tare Weight** | * **1350kg** |
| **ATM** | * **ATM – 3200KGS** |
| **Warranty (Subject to T&C’s)** | * **48 Month Structural Warranty** * **12 Months Fixtures & Fittings** * **12 Months Paint** * **Unregistered – Supplied with Blue Slip** |