
***A horse trailer parked on a road

Description automatically generatedA bus with a staircase

Description automatically generated with medium confidenceA trailer with open doors

Description automatically generatedA seat on a bus

Description automatically generated with medium confidence***

***2 HAL STANDARD – WARMBLOOD SQUARE - $27,995***

|  |  |
| --- | --- |
| **Specification** | * **2HAL – S SQUARE WB** |
| **Construction Materials** | * **Chassis: Double Hot Dip Galvanized RHS (Rectangular Hollow Section) (3.5mm-4.0mm)** * **Frame: Double Hot Dip Galvanized RHS (2.5mm)** * **Body Panels: Galvanized sheet (1.5mm)** * **Roof: Special Molded FRP (Fiber-reinforced Polymer - Glassfibre)** |
| **BRAKES** | * **Double Axle Electric Brakes, with Security Brake Away System, Rated to 1000kgs per Drum Brake.** |
| **DRAWBAR** | * **Drawbar Checker Plate 1.2mm High Strength Aluminium** * **Double Drawbar Safety Chains & One Bracing Wheel** |
| **Suspension** | * **7 Plate Roll Rocker Tandem Spring, With Grease Nipples** |
| **Axles** | * **Twin HD Trailer Axles 50\*50, rated to 2000kgs per axle** |
| **Wheels & Tyres** | * **5 x 185 R14 tyres with 14' aluminum alloy rims including a lockable spare wheel** |
| **Flooring & Rubber Matting** | * **Re-enforced Aluminium Flooring, Covered with 18-20mm Anti Slip Rubber** * **Rubber Matting For Inner Side Panel, 6mm Rubber Matting** * **Rubber Matting For Floor & Ramp Door, 18-20mm Anti-Slip Rubber Matting** |
| **Windows & Doors** | * **Front Window 1220x610mm** * **4 Side Sash Windows 600mmx400mm, With Fly Screens** * **2 large Push-up Roof Vents** * **Rear Upper Door 1980x1065mm. 2 x High-strength anti-rust struts** * **Ramp Door 2030x1210mm, with anti slip rubber matting** * **Side Door 1730x615mm** * **Hinges for Rear Upper Door - 6mm diameter Copper hinges** |
| **Supporting Wheel** | * **Swing-up HD Knight Dolly wheel** |
| **Lights& Retro Reflectors** | * **Trailer Plug - Seven prong** * **Aluminium Rear Lights Brackets** * **2 x LED interior lights, 2 x small LED sidelights, 2 x LED combination tail lights** * **8 x Retro Reflectors** |
| **Standard Auxiliary Fittings** | * **Fully Lined Roof** * **Padded Horse Protection Frame** * **Fully adjustable bays 2600mm long** * **4 x Horse Rings/Tie Ups** * **2 x Saddle Racks with Bridle Hooks** * **1 x Large Rug Rack** * **1 x Swing-out Tack Box** |
| **Dimensions** | * **Body Dimension (L x W x Hmm) : 4335 x 1980 x 2230** * **Inner Dimension (L x W x Hmm) : 4330 x 1930 x 2225** * **Overall Dimension (L x W x Hmm): 5185 x 2490 x 2670** |
| **Tare Weight** | * **1700kg Length of Tow: 850mm. Tow ball weight 260kgs** |
| **ATM** | * **3300kgs** |
| **Warranty (Subject to T&C’s)** | * **48 Month Structural Warranty** * **Unregistered – Supplied with Blue Slip** |