A close-up of a train

Description automatically generated***A ladder leading to a kitchen

Description automatically generated***

***2 HAL DELUXE – SQUARE $29,995***

|  |  |
| --- | --- |
| **Specification** | * **2 HAL LUX – SQUARE** |
| **Construction Materials** | * **Chassis: Double Hot Dip Galvanized RHS 3.5mm-4.0mm** * **Frame: Double Hot Dip Galvanized RHS (2.5mm)** * **Body Panels: Galvanized sheet (1.5mm)** * **Roof: Special Molded FRP Fiber-reinforced Polymer - Glassfibre (3mm)** |
| **BRAKES** | * **Double Axle Electric Brakes, with Security Brake Away System, rated to 1000kgs per Drum** |
| **DRAWBAR** | * **Drawbar Checker Plate 1.2mm High Strength Aluminium** * **Double Drawbar Safety Chains & One Bracing Wheel** |
| **Suspension** | * **7 Plate Roll Rocker Tandem Spring, With Grease Nipples** |
| **Axles** | * **Twin HD Trailer Axles 50\*50, rated to 2000kgs each.** |
| **Wheels & Tyres** | * **5 x 185 R14 tyres with 14' aluminum alloy rims including a lockable spare wheel** |
| **Flooring & Rubber Matting** | * **Re-enforced Aluminium Flooring, Covered with 18-20mm Anti Slip Rubber** * **Rubber Matting For Inner Side Panel, 6mm Rubber Matting** * **Rubber Matting For Floor & Ramp Door, 18-20mm Anti-Slip Rubber Matting** |
| **Windows & Doors** | * **Front Window 1220x610mm** * **2 Side Sash Windows 600mmx400mm, With Fly Screens** * **2 Drop down sliding windows, with fly screen** * **2 large Push-up Roof Vents** * **Rear Upper Door 1980x1065mm. 2 x High-strength anti-rust struts** * **Ramp Door 2030x1210mm, with anti slip rubber matting** * **Side Door 1730x615mm** * **Hinges for Rear Upper Door - 6mm diameter Copper hinges** |
| **Supporting Wheel** | * **Swing-up HD Knight Dolly wheel** |
| **Lights& Retro Reflectors** | * **Trailer Plug - Seven prong** * **Aluminium Rear Lights Brackets** * **2 x small LED sidelights, 2 x LED combination tail lights** * **8 x Retro Reflectors** |
| **Standard Auxiliary Fittings** | * **Padded Horse Protection Frame** * **4 x Horse Rings/Tie Ups** * **1 x swing out tack box** * **1 x Large Overhead Rug Rack** * **Fully adjustable bays 2400mm long** * **Premium front kitchen** * **2 x Fold up barrier beds** * **1 x top bunk 1900mm w x 900mm d** * **65L water tank, water pump, internal sink, interior and exterior tap** * **240v/12v power supply** * **Double Pole | 2 Double Sockets** |
| **Dimensions** | * **Body Dimension (L x W x Hmm) : 4120 x 1980 x 2230** * **Inner Dimension (L x W x Hmm) : 4070 x 1930 x 2155** * **Overall Dimension (L x W x Hmm): 4970 x 2490 x 2600** |
| **Tare Weight** | * **1800kg (tow ball weight 180kgs)** |
| **ATM** | * **ATM – 3,400kgs** |
| **Warranty (Subject to T&C’s)** | * **48 Month Structural Warranty** * **12 Months Fixtures & FittingsUnregistered – Supplied with Blue Slip** |